Same as 20090914 except with fixed clamp

calibrate-10a.log:
  Using the calibrate tool to get curves for keithley ±200mA.
  Effective with 50 turns is ±10A.

calibrate-50a.log:
  Same, keithley ±1A.



